SEAT WARMER UNIT INSPECTION

id091300716200

Seat Cushion

1. Remove the seat. (See SEAT REMOVAL/INSTALLATION.)

2. Remove the seat cushion trim. (See SEAT CUSHION TRIM REMOVAL/INSTALLATION.)

3. Connect a jumper wire to the connector for the seat cushion warmer to seat back warmer.

amxuuw00002074

4. While inspecting for continuity between the terminals A and B of the connector, use a dryer to warm the thermostat of the seat warmer unit on seat cushion.

amxuuw00002071

5. Verify that the continuity between the seat warmer terminals is as indicated in the table.

amxuuw00002072

  • If not as indicated in the table, replace the seat warmer unit.

  e5u913zw5004

Seat Back

1. Remove the seat. (See SEAT REMOVAL/INSTALLATION.)

2. Remove the seat back trim. (See SEAT BACK TRIM REMOVAL/INSTALLATION.)

3. Verify that the continuity between the seat warmer terminals is as indicated in the table.

amxuuw00002072

  • If not as indicated in the table, replace the seat warmer unit.

  amxuuw00002073