KEYLESS ENTRY SYSTEM OUTLINE

id091400593700

• The doors also can be locked/unlocked by operating the key or transmitter.
• The answer-back function has been adopted where the hazard warning lights flash and a buzzer sounds to confirm that the doors are locked/unlocked.
• A rolling code type transmitter has been adopted to prevent theft by radiowave interception.
• To prevent improper operation while the vehicle is moving, the doors cannot be locked/unlocked by operating the transmitter if the ignition key is not in the LOCK position.