DTC P0610 [L8, LF]

id0102b1809600

DTC P0610 | PCM vehicle options error
--- | ---
DETECTION CONDITION | • The PCM data configuration error. Diagnostic support note • This is a continuous monitor (CCM). • The MIL illuminates if the PCM detects the above malfunction condition during the first drive cycle. • FREEZE FRAME DATA (Mode 2/Mode 12) is available. • The DTC is stored in PCM memory.
POSSIBLE CAUSE | • Configuration procedure has not been completed • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA (MODE 12) HAS BEEN RECORDED • Has the FREEZE FRAME DATA (Mode 12) been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA (Mode 12) on the repair order, then go to the next step.
2 | VERIFY RELATED SERVICE INFORMATION AVAILABILITY • Verify related Service Information availability. • Is any related Service Information available? | Yes | Perform repair or diagnosis according to the available Service Information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | VERIFY PCM CONFIGURATION HAS BEEN PERFORMED • Perform the “PCM CONFIGURATION”. (See PCM CONFIGURATION [L8, LF].) • Turn the ignition switch to the ON position (engine off). • Start the engine and warm it up completely. • Clear the DTC from the PCM memory using the M-MDS. (See AFTER REPAIR PROCEDURE [L8, LF].) • Perform the KOEO/KOER self test. (See KOEO/KOER SELF TEST [L8, LF].) • Is the same DTC present? | Yes | Perform the “PCM CONFIGURATION” again, then go to the next step. (See PCM CONFIGURATION [L8, LF].)
No | Go to Step 5.
4 | VERIFY DTC TROUBLESHOOTING COMPLETED • Turn the ignition switch to the ON position (engine off). • Clear the DTC from the PCM memory using the M-MDS. (See AFTER REPAIR PROCEDURE [L8, LF].) • Start the engine and warm it up completely. • Perform the KOEO/KOER self test. (See KOEO/KOER SELF TEST [L8, LF].) • Is the same DTC present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION [L8, LF].)
No | Go to the next step.
5 | VERIFY AFTER REPAIR PROCEDURE • Perform the “AFTER REPAIR PROCEDURE”. (See AFTER REPAIR PROCEDURE [L8, LF].) • Are any DTCs present? | Yes | Go to the applicable DTC troubleshooting. (See DTC TABLE [L8, LF].)
No | DTC troubleshooting completed.