DECK PANEL MOTOR REMOVAL/INSTALLATION

id091600811300

  Caution
  • If the deck panel does not operate electrically, see “DECK PANEL MANUAL OPEN/CLOSE PROCEDURE” to open/close the deck panel. (See DECK PANEL MANUAL OPEN/CLOSE PROCEDURE)

1. Fully open the deck panel.

2. Remove the battery cover.

3. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

4. Set the side shelf out of the way. (See SIDE SHELF REMOVAL/INSTALLATION.)

5. Remove the deck panel. (See DECK PANEL REMOVAL/INSTALLATION.)

6. Remove the screws indicated in the figure.

amxzzw00000913

7. Disconnect the deck panel motor connector.

8. Remove the deck panel motor.

9. Install in the reverse order of removal.