REFRIGERANT PRESSURE SWITCH INSPECTION [MANUAL AIR CONDITIONER]

id0740a2802700

1. Connect the manifold gauge.

2. Verify the high-pressure side reading.

3. Disconnect the refrigerant pressure switch connector.

4. Verify continuity between the terminals of the refrigerant pressure switch.

  • If the continuity is not normal, replace the refrigerant pressure switch.

e5u711zw5a09

amxzzw00001139