HEATED OXYGEN SENSOR (HO2S) REMOVAL/INSTALLATION [L8, LF]

id0140i7804000

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Install the SST to the HO2S.

amxzzw00000126

4. Remove the HO2S.

5. Install in the reverse order of removal.

  HO2S tightening torque

  29—49 N·m {3.0—4.9 kgf·m, 22—35 ft·lbf}