INSTRUMENT CLUSTER SPECIFICATIONS

id092200532600

Item | Specification
--- | ---
Speedometer | Meter type | Stepping motor type
Input signal communication system | CAN system
Input signal source | PCM
Rated voltage | (V) | DC 12
Tachometer | Meter type | Stepping motor type
Input signal communication system | CAN system
Input signal source | PCM
Rated voltage | (V) | DC 12
Fuel gauge | Meter type | Stepping motor type (Reset-to-zero type)
Input signal communication system | Conventional communication system
Input signal source | Fuel gauge sender unit
Rated voltage | (V) | DC 12
Water temperature gauge | Meter type | Stepping motor type (Medium range stabilized type)
Input signal communication system | CAN system
Input signal source | PCM
Rated voltage | (V) | DC 12
Oil pressure gauge | Meter type | Stepping motor type
Input signal communication system | CAN system
Input signal source | PCM
Rated voltage | (V) | DC 12
Odometer/Tripmeter | Display | LCD
Indication digits | Odometer: 6 digits, Tripmeter: 4 digits
Input signal communication system | CAN system
Input signal source | PCM
Rated voltage | (V) | DC 12
Warning alarms | Sound frequency | (Hz) | 1,900—2,600
Output sound pressure level | (dB) | 53.5—67.5
Lights-on reminder warning alarm | Sound frequency | (Hz) | 1,900
Sound cycle |
Seat belt warning alarm | Sound frequency | (Hz) | 1,900
Sound cycle |
Tire pressure warning alarm | Sound frequency | (Hz) | 2,600
Sound cycle |
Power retractable hardtop warning alarm | Sound frequency | (Hz) | 1,900
Sound cycle | Operation start sound |
Operation complete sound |
Operation reject sound |
Warning |
Active bonnet warning alarm | Sound frequency | (Hz) | 2,200
Sound cycle |