REAR FLOOR PAN INSTALLATION [PANEL REPLACEMENT]

id098008742800

1. When joining and cutting the new and existing parts, trial fit the new part in position, then measure and adjust the body as necessary to conform with standard dimensions.

2. Cut area (A) on the new part.

3. Drill holes for plug welds before installing new parts.

4. Apply spot sealer to the areas where both the overlapping ends of the new and existing parts will be welded. Adhere the sections to be welded, and fillet weld along both seams at the locations indicated by (B).

  Note
  • Create a flange with flanging tool where new and existing parts are joined.

5. Weld the remaining weld locations and install the rear floor pan.

d5u0980b113

d5u0980b114