BUCKLE SWITCH INSPECTION

id081100803000

1. Turn the ignition switch to the LOCK position.

2. Remove the battery cover.

3. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

4. Disconnect the buckle switch connector.

5. Inspect for continuity between the buckle switch terminals using a tester.

amxzzw00001797

  • If not as indicated in the table, replace the buckle.

amxzzw00001798