ACTIVE BONNET CONTROL MODULE DISASSEMBLY/ASSEMBLY

id081300002900

  Warning
  • Handling the active bonnet control module improperly can cause it to accidentally operate, which could lead to serious injury. Read the service warnings and cautions before handling the active bonnet control module. (See ACTIVE BONNET SERVICE WARNINGS.) (See ACTIVE BONNET SERVICE CAUTIONS.)
  • After the active bonnet has deployed, always newly replace the parts indicated in the active bonnet service warnings in the section dealing with the active bonnet. If the vehicle is driven without part replacement, the active bonnet may not deploy correctly. (See ACTIVE BONNET SERVICE WARNINGS.)

1. Disassemble in the order shown in the figure.

amxzzw00002687

1 | Nut
2 | Bracket
3 | Active bonnet control module

2. Assemble in the reverse order of disassembly.