SUPPLIER IDENTIFICATION PROCEDURE [AUDIO]

id0902f6803800

  Note
  • The supplier can vary with the unit. When asking the supplier (service center) for repair or replacement, identify the supplier and fill in the Audio Repair Order Form with the following procedures.

Identification Using the Label or Inscribed Lettering

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the lower panel. (See LOWER PANEL REMOVAL/INSTALLATION.)

4. Remove the console. (See CONSOLE REMOVAL/INSTALLATION.)

5. Remove the side wall. (See SIDE WALL REMOVAL/INSTALLATION.)

6. Remove the center panel unit. (See CENTER PANEL UNIT REMOVAL/INSTALLATION.)

7. Verify the supplier by referring to the label attached to each unit.

Verify Using the Diagnostic Assist Function

1. Turn the ignition switch to the ACC or ON position.

2. Turn the audio unit power to ON.

3. While pressing the POWER/VOLUME switch, simultaneously press the RDM/PRESET switch 5 for With RDS (radio data system)/PRESET swn 5 without RDS (radio data system) 3 s or more.

With RDS (radio data system)

amxzzw00002450

Without RDS (radio data system)

amxzzw00002451

4. Identify the supplier code by referring to the display.

amxzzw00001113

Supplier code | Supplier name
--- | ---
01 | SANYO Automedia
02 | Panasonic
03 | Clarion
04 | Pioneer
05 | VISTEON

  Note
  • The supplier code can also be identified from the DTC displays screen.

  amxzzw00000782

5. Cancel the diagnostic assist function by either turning off the audio unit power or by turning the ignition switch to the LOCK position.