DTC P2135 [L8, LF]

id0102b1812100

DTC P2135 | TP sensor No.1/No.2 voltage correlation problem
--- | ---
DETECTION CONDITION | • The PCM compares the input voltage from TP sensor No.1 with the input voltage from TP sensor No.2 when the engine is running. If the difference is more than the specification, the PCM determines that there is a TP sensor No.1/No.2 voltage correlation problem. Diagnostic support note • This is a continuous monitor (CCM). • The MIL illuminates if the PCM detects the above malfunction condition during the first drive cycle. • FREEZE FRAME DATA (Mode 2/Mode 12) is available. • The DTC is stored in the PCM memory.
POSSIBLE CAUSE | • Throttle body connector or terminals malfunction • PCM connector or terminals malfunction • TP sensor No.1/No.2 malfunction • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA (MODE 12) HAS BEEN RECORDED • Has the FREEZE FRAME DATA (Mode 12) been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA (Mode 12) on the repair order, then go to the next step.
2 | VERIFY RELATED SERVICE INFORMATION AVAILABILITY • Verify related Service Information availability. • Is any related Service Information available? | Yes | Perform repair or diagnosis according to the available Service Information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | INSPECT THROTTLE BODY CONNECTOR AND TERMINALS • Turn the ignition switch off. • Disconnect the throttle body connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the connector or terminals, then go to Step 6.
No | Go to the next step.
4 | INSPECT PCM CONNECTOR AND TERMINALS • Disconnect the PCM connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the connector or terminals, then go to Step 6.
No | Go to the next step.
5 | INSPECT TP SENSOR NO.1/NO.2 • Reconnect the throttle body and PCM connectors. • Inspect the TP sensor No.1/No.2. (See THROTTLE POSITION (TP) SENSOR INSPECTION [L8, LF].) • Is there any malfunction? | Yes | Replace the throttle body, then go to the next step. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [L8, LF].)
No | Go to the next step.
6 | VERIFY DTC TROUBLESHOOTING COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the PCM memory using the M-MDS. (See AFTER REPAIR PROCEDURE [L8, LF].) • Start the engine and warm it up completely. • Perform the KOEO/KOER self test. (See KOEO/KOER SELF TEST [L8, LF].) • Is the same DTC present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION [L8, LF].)
No | Go to the next step.
7 | VERIFY AFTER REPAIR PROCEDURE • Perform the “AFTER REPAIR PROCEDURE”. (See AFTER REPAIR PROCEDURE [L8, LF].) • Are any DTCs present? | Yes | Go to the applicable DTC troubleshooting. (See DTC TABLE [L8, LF].)
No | DTC troubleshooting completed.