DOOR CHECKER REMOVAL/INSTALLATION

id091100602800

1. Disconnect the negative battery cable.(SeeBATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Remove the following parts:

  (1) Door trim (See DOOR TRIM REMOVAL/INSTALLATION.)

  (2) Door speaker (See DOOR SPEAKER REMOVAL/INSTALLATION.)

3. Remove the bolt.

amxzzw00000214

4. Remove the nut.

amxzzw00000215

5. Pull out the door checker from the door speaker installation hole.

6. Install in the reverse order of removal.