SEAT WARMER SWITCH REMOVAL/INSTALLATION

id091300716000

1. Turn the ignition switch to LOCK position.

2. Remove the battery cover.

3. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

4. Remove the console. (See CONSOLE REMOVAL/INSTALLATION.)

5. Remove the side wall. (See SIDE WALL REMOVAL/INSTALLATION.)

6. Remove the console panel. (See CONSOLE PANEL REMOVAL/INSTALLATION.)

7. Squeeze the tabs of seat warmer switch in the direction of arrow shown in the figure, and pull it outward to remove it.

amxzzw00001503

8. Install in the reverse order of removal.