AIR DIST UNIT DISASSEMBLY/ASSEMBLY

id071100807000

1. Disassemble in the order indicated in the table.

  Caution
  • If a non-specified grease is used, it may result in abnormal noise or improper operation of the links. Apply only the specified grease to each link.

L.H.D.

amxzzw00002064

R.H.D.

amxzzw00002065

1 | Duct (1)
2 | Duct (2)
3 | Airflow mode actuator
4 | Bracket
5 | Airflow mode main link
6 | Airflow mode link set
7 | Airflow mode door
8 | Polyurethane form
9 | Case (1)
10 | Case (2)

2. Assemble in the reverse order of disassembly.