NEUTRAL SWITCH INSPECTION [L8, LF]

id0140i7800800

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Disconnect the negative battery cable.

3. Remove the neutral switch. (See NEUTRAL SWITCH REMOVAL/INSTALLATION [M15M-D].) (See NEUTRAL SWITCH REMOVAL/INSTALLATION [P66M-D].)

4. Inspect for continuity between the neutral switch terminals using an ohmmeter.

am6xuw00001347

  • If not as specified, replace the neutral switch.
  (See NEUTRAL SWITCH REMOVAL/INSTALLATION [M15M-D].) (See NEUTRAL SWITCH REMOVAL/INSTALLATION [P66M-D].)

Specification

Measured condition | Continuity
--- | ---
Rod pushed | Continuity detected
Except above | No continuity