CONSOLE PANEL REMOVAL/INSTALLATION

id091700718200

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the console. (See CONSOLE REMOVAL/INSTALLATION.)

4. Remove the side wall. (See SIDE WALL REMOVAL/INSTALLATION.)

5. Remove the screws.

amxzzw00001409

6. Pull the console panel outward and detach tabs A and pins B.

7. Disconnect the seat warmer switch connector. (Vehicles with seat warmer)

8. Disconnect the accessory socket connector.

9. Disconnect the auxiliary jack connector.

10. Remove the console panel.

11. Install in the reverse order of removal.