GENERAL PROCEDURES (CLUTCH)

id051000800500

  Caution
  • Fluid will damage painted surfaces. Be careful not to spill any fluid on painted surfaces. If fluid does get on painted surfaces, wipe it off immediately.

  Note
  • If any hydraulic related parts of the clutch sytem are removed during the procedure, add brake fluid, bleed the system and inspect for leakage after the procedure has been completed.

1. Remove the clutch pipe.

2. Install the clutch pipe using a torque wrench.