PARKING BRAKE LEVER INSPECTION

id041200800900

Stroke Inspection

1. Depress the brake pedal several times.

2. Pull the parking brake lever 2—3 times.

3. Inspect the parking brake stroke by slowly pulling at point A 50 mm {1.97 in} from the end of the parking brake lever with a force of 98 N {10 kgf, 22 lbf} and counting the number of notches (clicking sound).

e5u412zw5002

  • If not within the specification, adjust the parking brake lever.

  Parking brake lever stroke when pulled at 98 N {10 kgf, 22 lbf}

  1—3 notches