VARIABLE INTAKE AIR SOLENOID VALVE REMOVAL/INSTALLATION [L8, LF]

id0113a3805500

1. Remove the plug hole plate. (See PLUG HOLE PLATE REMOVAL/INSTALLATION [L8, LF].)

2. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

4. Move the variable tumble solenoid valve slightly out of the way. (See VARIABLE TUMBLE SOLENOID VALVE REMOVAL/INSTALLATION [L8, LF].)

5. Remove in the order indicated in the table.

6. Install in the reverse order of removal.

amxzzw00000902

1 | Connector
2 | Vacuum hose
3 | Variable intake air solenoid valve