THEFT-DETERRENT SYSTEM OUTLINE

id091400599000

• The theft-deterrent system includes sound and light alarms that activate when the bonnet, the trunk lid or a door is opened by means other than the transmitter. The turn lights flash and the horn and the theft-deterrent siren sound
• When the transmitter unlock button is pressed, the alarms stop.
• An intruder sensor has been installed in the rear part of the console. The intruder sensor senses movement in the vehicle based on radio waves, and sends an alert signal to the keyless control module.
• A theft-deterrent siren has been installed on the rear, left side of the trunk. The theft-deterrent siren includes an internal back-up power supply so that if power from the battery is cut by any means, the siren will still sound.