GENERATOR CONSTRUCTION [L8, LF]

id0117a6102300

• With the elimination of the voltage regulator, generator control is carried out by the PCM. Excitation current in the field coil is increased or decreased by the duty signal from the PCM sent to the power transistor built into the generator. (See GENERATOR CONTROL OUTLINE [L8, LF].)
• Two delta connection type stator coils have been adopted.
• A generator duct and a generator heat insulator have been adopted to protect the generator from the exhaust manifold heat.

amxzzn00000569

amxzzn00000570

• The phase difference in the circuit of the two stator coils causes the electromagnetic pull between the rotor and the stator to be eliminated logically. Due to this, electromagnetic vibration and generator operation noise (electromagnetic noise) have been reduced.

amxzzn00000571

• The pulsation occurring through voltage rectifying is minimized, as a result, stable voltage output is supplied due to the adoption of two stator coils with the phase difference.

amxzzn00000572

• If there is malfunction in the charging system, the generator warning light in the instrument cluster illuminates. (See ON-BOARD DIAGNOSTIC SYSTEM TEST MODE [L8, LF].)