DOOR QUARTER GLASS REMOVAL/INSTALLATION

id091200813200

1. Position the door glass so that the distance between the top of the front door glass and top of the front beltline molding is 110 mm {4.33 in}.

e5u912zw5002

2. Remove the battery cover.

3. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

4. Remove the door trim. (See DOOR TRIM REMOVAL/INSTALLATION.)

5. Remove the door module panel. (See DOOR MODULE PANEL REMOVAL/INSTALLATION.)

6. Remove the door glass. (See DOOR GLASS REMOVAL/INSTALLATION.)

7. Remove the power window regulator. (See POWER WINDOW REGULATOR REMOVAL/INSTALLATION.)

8. Remove the nut and bolt, then remove the door glass guide. (See Door Glass Guide Installation Note.)

e5u912zw5043

9. Remove the nuts, then remove the door quarter glass.

e5u912zw5044

10. Install in the reverse order of removal.

Door Glass Guide Installation Note

1. Adjust the adjustment bolt as shown in the figure.

e5u912zw5064