NO.3 VEHICLE MOVES IN P POSITION, OR PARKING GEAR DOES NOT DISENGAGE WHEN P IS DISENGAGED [SJ6A-EL]

id050307800800

3 | Vehicle moves in P position, or parking gear does not disengage when P is disengaged
DESCRIPTION | • Vehicle rolls when on a downward slope and tires do not lock in P position. • Tires are locked when P is disengaged. Vehicle does not move in D range, and R position when the accelerator pedal is depressed, and the engine remains in a stalled condition.
POSSIBLE CAUSE | • Parking mechanism malfunction (May have effect on noise or shock from transmission) • Selector lever malfunction • If the vehicle moves in N position, perform the symptom troubleshooting “NO.2 VEHICLE MOVES IN N POSITION”. (See NO.2 VEHICLE MOVES IN N POSITION [SJ6A-EL].)