SYMPTOM TROUBLESHOOTING [INSTRUMENT CLUSTER]

id0903d5807200

No. | TROUBLESHOOTING ITEM | PAGE
--- | --- | ---
1 | Fuel gauge needle position incorrect | (See NO. 1 FUEL GAUGE NEEDLE POSITION INCORRECT [INSTRUMENT CLUSTER].)
2 | All meters and gauges do not operate | (See NO. 2 ALL METERS AND GAUGES DO NOT OPERATE [INSTRUMENT CLUSTER].)
3 | ABS warning light illuminates | (See NO. 3 ABS WARNING LIGHT ILLUMINATES [INSTRUMENT CLUSTER].)
4 | MIL illuminates | (See NO. 4 MIL ILLUMINATES [INSTRUMENT CLUSTER].)
5 | Brake system warning light illuminates | (See NO. 5 BRAKE SYSTEM WARNING LIGHT ILLUMINATES [INSTRUMENT CLUSTER].)
6 | Instrument cluster illumination does not illuminate | (See NO. 6 INSTRUMENT CLUSTER ILLUMINATION DOES NOT ILLUMINATE [INSTRUMENT CLUSTER].)
7 | Speedometer indication is defective | (See NO. 7 SPEEDOMETER INDICATION IS DEFECTIVE [INSTRUMENT CLUSTER].)
8 | Tachometer indication is defective | (See NO. 8 TACHOMETER INDICATION IS DEFECTIVE [INSTRUMENT CLUSTER].)
9 | Water temperature gauge indication is defective | (See NO. 9 WATER TEMPERATURE GAUGE INDICATION IS DEFECTIVE [INSTRUMENT CLUSTER].)
10 | Oil pressure gauge indication is defective (oil pressure gauge needle does not move from the L position or less) | (See NO. 10 OIL PRESSURE GAUGE INDICATION IS DEFECTIVE (OIL PRESSURE GAUGE NEEDLE DOES NOT MOVE FROM THE L POSITION OR LESS) [INSTRUMENT CLUSTER].)
11 | Malfunction warning light illuminates | (See NO. 11 MALFUNCTION WARNING LIGHT ILLUMINATES [INSTRUMENT CLUSTER].)