DTC INSPECTION [INSTRUMENT CLUSTER]

id0902e8960300

1. Connect the M-MDS to the DLC-2.

amxzzw00000867

2. After the vehicle is identified, select the following items from the initialization screen of the M-MDS.

  • When using the IDS (laptop PC)
    1. Select “Self Test”.
    2. Select “Modules”.
    3. Select “IC”.

  • When using the PDS (Pocket PC)
    1. Select “Module Tests”.
    2. Select “IC”.
    3. Select “Self Test”.

3. Verify the DTC according to the directions on the screen.

  • If any DTCs are displayed, perform troubleshooting according to the corresponding DTC inspection.

4. After completion of repairs, clear all DTCs stored in the instrument cluster. (See CLEARING DTC [INSTRUMENT CLUSTER].)