SELECTOR LEVER COMPONENT INSPECTION

id051400255600

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the shift knob. (See SELECTOR LEVER REMOVAL/INSTALLATION.)

4. Remove the console panel and indicator assembly. (See SELECTOR LEVER REMOVAL/INSTALLATION.)

5. Disconnect the selector lever component connector.

6. Verify continuity as indicated in the table.

amxzzw00000213

  • If there is any malfunction, replace the selector lever. (See SELECTOR LEVER REMOVAL/INSTALLATION.)

amxzzw00000282