PLUG HOLE PLATE REMOVAL/INSTALLATION [L8, LF]

id0110a9803900

1. Remove the plug hole plate.

  Note
  • Lift off and remove the plug hole plate from the installation areas (rubber and clips) as shown in the figure.

  e5u110zw5105

  a6a4712w301

2. Install the plug hole plate.

  (1) To position the plug hole plate, grasp rubber 1 and 2, as shown in the figure, with your hands and press them in.

  e5u110zw5106

  (2) Grasp clips 3 with your hands and press them in.