ON-BOARD DIAGNOSTIC SYSTEM ACTIVE COMMAND MODES FUNCTION [ABS]

id0402a7181500

• The active command modes function is used for optionally selecting active command modes items of input/output parts preset in the ABS HU/CM, and to operate them regardless of CM control.
• To protect the hydraulic unit interior, operate output related parts for only 10 s or less when using the active command modes function.

Active Command Modes Table

Command name | Output part name | Operation | Operation condition
--- | --- | --- | ---
LF_INLET | LF inlet solenoid valve | Off/On | Ignition switch at ON
LF_OUTLET | LF outlet solenoid valve
LR_INLET | LR inlet solenoid valve
LR_OUTLET | LR outlet solenoid valve
PMP_MOTOR | Pump motor
RF_INLET | RF inlet solenoid valve
RF_OUTLET | RF outlet solenoid valve
RR_INLET | RR inlet solenoid valve
RR_OUTLET | RR outlet solenoid valve