COMBINED SENSOR REMOVAL/INSTALLATION

id041500801200

  Caution
  • The internal parts of the combined sensor could be damaged if dropped. Be careful not to drop the combined sensor. Replace the combined sensor if it is subjected to an impact. Also, do not use an impact wrench or other similar air tools when removing/installing the sensor.

1. Remove the console. (See CONSOLE REMOVAL/INSTALLATION.)

2. Remove in the order indicated in the table.

amxzzw00002027

1 | Combined sensor connector (See Combined Sensor Connector Installation Note.)
2 | Nut
3 | Combined sensor
4 | Bracket

3. Install in the reverse order of removal.

4. After installation, perform the combined sensor initialization procedure. (See STEERING ANGLE SENSOR INITIALIZATION PROCEDURE.)

Combined Sensor Connector Installation Note

1. Connect the combined sensor connector to the combined sensor until a click is heard.