DECK PANEL LINK CONSTRUCTION/OPERATION

id091600101600

Construction

• The links rise according to the rotation of the deck panel links to fully open or close the deck panel.
• The deck panel limit switch is installed to the deck panel link (RH).
• The guide for the deck panel manual open/close is installed to the deck panel base link. (Refer to the Workshop Manual for the procedure.)

amxzzn00000604

Operation

1. The deck panel motor starts to rotate based on an operation signal of the power retractable hardtop control module.

2. The sector gear rotates according to the deck panel motor rotation, and the lock pin area of the deck panel base link and sector gear are disengaged.

amxzzn00000605

3. The knob presses deck panel link A upward by the rotation of the sector gear.

amxzzn00000606

4. Deck panel link A is pressed upward to fully open the deck panel.

amxzzn00000607

5. When deck panel link A is fully opened, the sector gear pin shown in the figure presses the deck panel open position switch to stop the deck panel motor rotation.

amxzzn00000608