HINGE PILLAR (OUTER) INSTALLATION [PANEL REPLACEMENT]

id098008613600

1. When joining and cutting the new and existing parts, trial fit the new part in position, then measure and adjust the body as necessary to conform with standard dimensions.

2. Drill holes for plug welds before installing new parts.

3. After temporarily installing new parts, make sure the related parts fit properly.

4. Install the front pillar (inner).

d5u0980b078

5. Install the front pillar reinforcement.

d5u0980b079

6. Install the cowl side panel.

d5u0980b080

7. Install the hinge pillar (outer).

d5u0980b081