BLOWER MOTOR REMOVAL/INSTALLATION [FULL-AUTO AIR CONDITIONER]

id0740a1800900

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the front side trim. (R.H.D.)(See FRONT SIDE TRIM REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

L.H.D.

e5u740zw5007

R.H.D.

amxzzw00000975

1 | Blower motor connector
2 | Blower motor

5. Install in the reverse order of removal.