PARKING BRAKE LEVER REMOVAL/INSTALLATION

id041200801600

1. Remove the middle pipe. (See EXHAUST SYSTEM REMOVAL/INSTALLATION [L8, LF].)

2. Remove the propeller shaft. (See PROPELLER SHAFT REMOVAL/INSTALLATION.)

3. Remove the console. (See CONSOLE REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

5. Install in the reverse order of removal.

6. After installation, inspect the parking brake stroke and adjust if necessary.

amxzzw00000253

1 | Parking brake switch connector
2 | Adjusting nut
3 | Parking brake lever (See Parking Brake Lever Removal Note.)
4 | Parking brake switch
5 | Clip
6 | Rear parking brake cable (LH)
7 | Rear parking brake cable (RH)
8 | Front parking brake cable

Parking Brake Lever Removal Note

1. Partially peel back the floor mat and remove the bolt shown in the figure.

amxzzw00000254

2. Remove the two bolts.

3. Remove the parking brake lever.