SEAT BELT WARNING ALARM CONSTRUCTION/OPERATION

id092200101800

System Wiring Diagram

amxzzn00000628

Operation

• If all of the following conditions are met, a beeper sounds intermittently as shown in the table.

  ― The seat belt (driver side or passenger side) is unfastened (driver side: buckle switch is on, passenger side: buckle switch is on and occupancy sensor detects passenger).
  ― Initialization warning: Vehicle speed is approx. 15—20 km/h {9.4—12.0 mph} or more.
  ― Recurrent warning: Vehicle speed is approx. 15—20 km/h {9.4—12.0 mph} or more.

Initialization warning

Initial warning | 6—8 s
Intermediate warning | 22—24 s
Main warning | 92—94 s

Recurrent warning

Initial warning | 6—8 s
Intermediate warning | 7—9 s
Main warning | 92—94 s