DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)]

id0902j3845800

HS-CAN

DTC Output Unit (M-MDS display) | DTC | Malfunction location | Reference for inspection procedure
--- | --- | --- | ---
PCM (PCM) | U0073*1 | CAN system communication error | (See DTC U0001:88, U0073, U1900 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0101 | Communication error to TCM | (See DETERMINING MALFUNCTIONING PART (HS-CAN) [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0121 | Communication error to ABS HU/CM (With ABS) Communication error to DSC HU/CM (With DSC)
U0155 | Communication error to instrument cluster
TCM*2 (TCM) | U0073*1 | CAN system communication error | (See DTC U0001:88, U0073, U1900 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0100 | Communication error to PCM | (See DETERMINING MALFUNCTIONING PART (HS-CAN) [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
ABS HU/CM*3 (ABS) | U0073*1 | CAN system communication error | (See DTC U0001:88, U0073, U1900 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U1900*1 | Communication error to other module
U2023 | Abnormal message from PCM | (See DTC U2023 [ABS].)
DSC HU/CM*4 (ABS) | U0073*1 | CAN system communication error | (See DTC U0001:88, U0073, U1900 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0100 | Communication error to PCM | (See DETERMINING MALFUNCTIONING PART (HS-CAN) [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0101 | Communication error to TCM
U0155 | Communication error to instrument cluster
U1900*1 | Communication error to other module | (See DTC U0001:88, U0073, U1900 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U2023 | Abnormal message from PCM | (See DTC U2023 [DYNAMIC STABILITY CONTROL (DSC)].)
Power retractable hardtop control module*5 (RHT) | U0073*1 | CAN system communication error | (See DTC U0001:88, U0073, U1900 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0100 | Communication error to PCM | (See DETERMINING MALFUNCTIONING PART (HS-CAN) [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0101 | Communication error to TCM
U2197 | Vehicle speed signal communication error
Active bonnet control module*6 (DHS) | U0001:88*1 | CAN system communication error | (See DTC U0001:88, U0073, U1900 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0155:00 | Communication error to instrument cluster | (See DETERMINING MALFUNCTIONING PART (HS-CAN) [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
Instrument cluster (IC) | U0073*1 | Module communication error | (See DTC U0001:88, U0073, U1900 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0100 | Communication error to PCM | (See DETERMINING MALFUNCTIONING PART (HS-CAN) [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
U0101 | Communication error to TCM
U0121 | Communication error to ABS HU/CM (With ABS) Communication error to DSC HU/CM (With DSC)
U0207 | Communication error to power retractable hardtop control module
U0214 | Communication error to keyless control module
U0250 | Communication error to active bonnet control module
U2023 | Abnormal message from PCM | (See DTC U2023 [INSTRUMENT CLUSTER].)
U2197 | Vehicle speed signal communication error | (See DETERMINING MALFUNCTIONING PART (HS-CAN) [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)

*1 :If only the target DTCs are displayed, perform the corresponding DTC inspection without determining the open circuit location.
*2 :AT
*3 :with ABS
*4 :with DSC
*5 :with power retractable hardtop
*6 :with active bonnet

MS-CAN

DTC Output Unit | DTC | Malfunction location | Reference for inspection procedure
--- | --- | --- | ---
Audio unit | 16:Er12*1 | Communication error between audio unit and HF/TEL unit | (See DTC 16:Er12 [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)
HF/TEL unit | 26:Er81 | CAN system communication error | (See DETERMINING MALFUNCTIONING PART (MS-CAN) [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].)

*1 :If only the target DTCs are displayed, perform the corresponding DTC inspection without determining the open circuit location.