STEERING SHIFT SWITCH INSPECTION

id051400255900

1. Remove the battery cover.

2. Disconnect the negative battery cable.

3. Disconnect the audio control switch connector. (See AUDIO CONTROL SWITCH REMOVAL/INSTALLATION.)

4. Measure resistance between the terminals F and C.

ar8wzw00000218

Test condition | Resistance (ohm) | Action
--- | --- | ---
Steering shift switch off | 1,764—1,836 | • Replace the audio control switch. (See AUDIO CONTROL SWITCH INSPECTION.)
LH up-switch on | 266.3—277.1 | • If not within the specification, replace the audio control switch. (See AUDIO CONTROL SWITCH INSPECTION.) • If there is no continuity, replace the up switch. (See AUDIO CONTROL SWITCH INSPECTION.)
RH up-switch on | 266.3—277.1
LH down-switch on | 452.0—470.3 | • Replace the audio control switch. (See AUDIO CONTROL SWITCH INSPECTION.)
RH down-switch on | 452.0—470.3