REVERSE LOCKOUT MECHANISM CONSTRUCTION/OPERATION [P66M-D]

id051111103900

• With the adoption of the reverse lockout mechanism, which utilizes a guide plate, reliability has been assured.
• A guide plate, attached to the extension housing, prevents accidental shifting into reverse when shifting from neutral to 1st gear by restricting the movement of the shift lever. When shifting into reverse, once the shift lever is pressed down and moved towards the reverse position, the projection on the lever goes under the guide plate, releasing the reverse shift restriction and allowing for shifting into reverse.

amxzzn00000201