REAR SIDE TRIM REMOVAL/INSTALLATION

id091700806000

Except Power Retractable Hardtop

1. Remove the following parts:

  (1) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (2) Quarter trim (See QUARTER TRIM REMOVAL/INSTALLATION.)

  (3) Scuff plate (See SCUFF PLATE REMOVAL/INSTALLATION.)

  (4) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)

  (5) Aeroboard (See AEROBOARD REMOVAL/INSTALLATION.)

  (6) Front seat back bar garnish (See SEAT BACK BAR GARNISH REMOVAL/INSTALLATION.)

  (7) Back trim (See BACK TRIM REMOVAL/INSTALLATION.)

  (8) Seat belt set plate (See SEAT BELT REMOVAL/INSTALLATION.)

  (9) Seat back crossmember assembly (See SEAT BACK CROSSMEMBER ASSEMBLY REMOVAL/INSTALLATION.)

2. Remove the fasteners.

e5u917zw5032

3. Pull the rear side trim outward and detach pin A, B and tab C.

4. Remove the rear side trim.

5. Install in the reverse order of removal.

Power Retractable Hardtop

1. Remove the following parts:

  (1) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (2) Quarter trim (See QUARTER TRIM REMOVAL/INSTALLATION.)

  (3) Scuff plate (See SCUFF PLATE REMOVAL/INSTALLATION.)

  (4) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)

  (5) Aeroboard (See AEROBOARD REMOVAL/INSTALLATION.)

  (6) Front seat back bar garnish (See SEAT BACK BAR GARNISH REMOVAL/INSTALLATION.)

  (7) Back trim (See BACK TRIM REMOVAL/INSTALLATION.)

2. Disconnect the power retractable hardtop drain hose. (See POWER RETRACTABLE HARDTOP DRAIN HOSE REMOVAL/INSTALLATION.)

3. Remove the fasteners.

amxzzw00001415

4. Remove the clip A and pin.

5. Remove the rear side trim.

6. Install the reverse order of removal.