NO.21 NOISE OCCURS AT IDLE WHEN VEHICLE IS STOPPED IN D RANGE, OR IN R POSITION [SJ6A-EL]

id050307802600

21 | Noise occurs at idle when vehicle is stopped in D range, or in R position
DESCRIPTION | • Transmission is noisy in driving ranges when vehicle is idling.
POSSIBLE CAUSE | • Although the malfunction is basically the same as “NO.20 NOISE OCCURS AT IDLE WHEN VEHICLE IS STOPPED IN ALL POSITIONS/RANGES”, other causes may include selector lever position disparity or TR switch position disparity. (See NO.20 NOISE OCCURS AT IDLE WHEN VEHICLE IS STOPPED IN ALL POSITIONS/RANGES [SJ6A-EL].)