REVERSE LOCKOUT MECHANISM CONSTRUCTION/OPERATION [M15M-D]

id051110103900

• A cam-type reverse lockout mechanism is adopted to ensure reliability.
• A cam, which is installed to the shift guide plate in the shift control case, restricts the selector movement to prevent the driver from miss shifting.
• When shifting into reverse, by shifting the selector back into the neutral position once and then shifting to the 5th/reverse direction, the selector pushes the cam outward to release the shifting restriction, and shifting into reverse is made possible.

Shift guide component operation

amxzzn00000187