THEFT-DETERRENT SIREN REMOVAL/INSTALLATION

id091400809500

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Remove the following parts:

  (1) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (2) Partition board (See PARTITION BOARD REMOVAL/INSTALLATION.)

  (3) Trunk side trim (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

3. Remove the nuts, then remove the theft-deterrent siren.

amxzzw00000576

4. Install in the reverse order of removal.