REAR BUMPER REMOVAL/INSTALLATION

id091000800700

1. Disconnect the negative battery cable. (SeeBATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Remove the following parts:

  (1) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (2) Partition board (See PARTITION BOARD REMOVAL/INSTALLATION.)

  (3) Trunk side trim (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

  (4) Rear combination lights (See REAR COMBINATION LIGHT REMOVAL/INSTALLATION.)

3. Remove the screws.

e5u910zw1017

4. Splash shield, detach tabs A, and then remove the splash shield.

5. Remove in the order indicated in the table.

amxzzw00001498

1 | Screw A
2 | Screw B
3 | Screw C
4 | Fastener A
5 | Energy absorbing form
6 | Rear bumper (See Rear Bumper Removal Note.) (See Rear bumper Installation Note.)

6. Install in the reverse order of removal.

Rear Bumper Removal Note

1. Affix the protective tape to the position shown in the figure.

amxzzw00002469

2. Pull the rear bumper ends (wheel arch) outward to detach from the bumper slider.

  Caution
  • When detaching the rear bumper from the bumper slider, the rear bumper could fall and be damaged. Secure the rear bumper so that it does not fall.

amxzzw00001906

Rear bumper Installation Note

1. Spread the rear bumper ends (wheel arches) apart.

2. Attach the rear bumper to the body.

3. Press the rear bumper connecting area into the body to engage with the bumper slider.