TORQUE CONVERTER REMOVAL/INSTALLATION [SJ6A-EL]

id051311710100

1. Remove the transmission. (See AUTOMATIC TRANSMISSION REMOVAL/INSTALLATION [SJ6A-EL].)

  Caution
  • The oil seal is easily damaged by the sharp edges of the torque converter splines. Do not let the splines contact the oil seal.
  • Do not drop the torque converter.
  • Do not pinch fingers.

2. Remove the torque converter, and immediately turn it so that the hole faces upward. This will help to keep any remaining ATF from spilling.

e5u513zw5040

3. Drain any ATF remaining in the torque converter.

4. Using a flathead screwdriver, position the drive gear on the oil pump component in the center.

5. Install the torque converter to the transmission.

e5u513zw5040

6. To ensure that the torque converter is installed accurately, measure distance A between the end of the torque converter and the end of the converter housing.

e5u513zw5039

  Distance A between end of torque converter and face of converter housing

  26.2 mm {1.03 in}

7. Install the automatic transmission. (See AUTOMATIC TRANSMISSION REMOVAL/INSTALLATION [SJ6A-EL].)

8. Perform the mechanical system test. (See MECHANICAL SYSTEM TEST [SJ6A-EL].)