GENERATOR REMOVAL/INSTALLATION [L8, LF]

id0117a6800200

  Warning
  • Remove and install all parts when the engine is cold, otherwise they can cause severe burns or serious injury.
  • When the battery cables are connected, touching the vehicle body with generator terminal B will generate sparks. This can cause personal injury, fire, and damage to the electrical components. Always disconnect the negative battery cable before performing the following operation.

  Caution
  • The generator can be damaged by the heat from the exhaust manifold. Make sure the generator duct is installed securely.

1. Remove the battery and battery tray. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Remove the drive belt. (See DRIVE BELT REPLACEMENT [L8, LF].)

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

e5u117zw5003

1 | P/S pressure hose bracket
2 | Generator bracket
3 | Generator duct
4 | Terminal B cable
5 | Generator connector
6 | Generator (See Generator Installation Note.)

Generator Installation Note

1. Tighten bolt A temporarily.

2. Tighten bolt B, C to the specified tightening torque.

3. Tighten bolt A to the specified tightening torque.