AIR FUEL RATIO (A/F) SENSOR REMOVAL/INSTALLATION [L8, LF]

id0140i7899700

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Install the SST to the A/F sensor.

amxzzw00000043

4. Remove the A/F sensor.

5. Install in the reverse order of removal.

  A/F sensor tightening torque

  29—49 N·m {3.0—4.9 kgf·m, 22—35 ft·lbf}