TRUNK LID OPENER REMOVAL/INSTALLATION

id091400812100

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Remove the trunk end trim. (See TRUNK END TRIM REMOVAL/INSTALLATION.)

3. Detach the rod.

4. Disconnect the trunk lid opener connector and the trunk compartment light connector.

e5u914aw4010

5. Remove the bolts, then remove the trunk lid opener.

6. Install in the reverse order of removal.