INSPECTION OF SST (DEPLOYMENT TOOL)

id081300001300

1. Before using the SST (49 H066 002), inspect its operation.

amxzzw00001785

Inspection procedure

1. Follow the steps below to inspect the SST (49 H066 002).

  • If not as indicated in the table, replace the SST (49 H066 002) because it has a malfunction.

  Warning
  • Do not use a malfunctioning SST, otherwise it could cause the active bonnet actuator to accidentally deploy.

  Caution
  • Because the permissible voltage for the SST (49 H066 002) is 12 V, connecting a 24 V power source could damage the SST. Always connect only a 12 V power supply.

Step | Inspection procedure | Illumination status
--- | --- | ---
Green | Red
1 | Connect the power supply red clip to the positive battery terminal, and the black clip to the negative battery terminal. | On | Off
2 | Connect connectors A and B. | Off | On
3 | Press the activation switch. | On | Off

e5u810zw5050