SERVICE PRECAUTIONS

id000000739200

Arrangement of Workshop

• Arrangement of the workshop is important for safe and efficient work.

Safety Precautions

• Protective head covering and safety shoes should always be worn. Depending upon the nature of the work, gloves, safety glasses, ear protectors, face shield, etc., should also be used.

mzz2036b001

Vehicle Protection

• Use seat covers and floor covers.
• Use heat‐resistant protective covers to protect glass areas and seats from heat or sparks during welding.
• Protect items such as moldings, garnishes, and ornaments with tape when welding.

mzz2036b002

Remove Dangerous Articles

• Remove the fuel tank before using an open flame in that area. Plug connection piping to prevent fuel leakage.

mzz2036b003

Use of Pulling Equipment

• When using pulling equipment, keep away from the pulling area and use safety wires to prevent accidents.

mzz2036b004

Prevent Short Circuits

• Turn the ignition switch to the LOCK position.
• Disconnect the battery cables.

mzz2036b005

  Note
  • When connecting the negative battery cable to the battery, connect the negative battery cable and the ground cable as shown in the figure.

  e5u117zw5004

• Securely connect the welding machine ground near the welding area.

mzz2036b006