POWER WINDOW SYSTEM PRELIMINARY INSPECTION [POWER WINDOW SYSTEM]

id0903a0831700

Manual Open/close Function Inspection

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Turn the ignition switch to the ON position. • Operate the driver’s side power window using the manual open/close function on the power window main switch. • Does the driver’s side power window operate properly? | Yes | Go to the next step.
No | • Inspect the following items: ― Power window main switch power supply fuse ― Power window main switch ground wiring harness ― Power window main switch power supply wiring harness ― Wiring harness between power window main switch and driver-side power window motor ― Power window main switch (driver’s-side power window control is malfunctioning) ― Driver-side power window motor • Repair or replace the malfunctioning part, then go to the next step.
2 | • Operate the passenger’s side power window using the power window main switch. • Does the passenger’s side power window operate properly? | Yes | • Manual open/close function is normal. • Perform the auto open/close function inspection.
No | • Inspect the following items: ― Wiring harness between power window main switch and passenger’s-side power window motor ― Power window main switch (passenger’s-side power window control is malfunctioning) ― Passenger-side power window motor • Repair or replace the malfunctioning part, then go to the next step.

Auto Open Function Inspection

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Turn the ignition switch to the ON position. • Operate the power window using the auto open function on the power window main switch. • Do each the driver’s power window operate properly? | Yes | Go to the next step.
No | • Go to No.1 THE AUTO OPEN FUNCTION ON THE DRIVER'S AND PASSENGER'S SIDE POWER WINDOW IS INOPERATIVE [POWER WINDOW SYSTEM].)
2 | • Operate the power window main switch to the close position while the power window is opening. • Does the power window operation stop? | Yes | • Auto open/close function is normal. • Perform the IG-OFF timer function inspection.
No | • Replace the power window main switch (power window control unit is malfunctioning.)